# Croky_b Setup Config Ver.5.5

Action 1 :
Action 2 :
Action 3 :
Action 4 :
Action 5 :
Action 6 :
Action 7 :
Action 8 :

Action 9 :
Action 10 :
Action 11 :
Action 12 :
Sequence1 :
Sequence1B :
Sequence2 :
Sequence2B :

led1 :
led2 :
led3 :
led4 :
led5 :
led6 :
led7 :
led8 :
led9 :
led10 :
led11 :
led12 :
led13 :
led14 :

Flash1 :
Flash2 :
Flash3 :
Flash4 :
Flash5 :
Flash6 :
Flash7 :
Flash8 :
Flash9 :
Flash10 :
Flash11 :
Flash12 :
Flash13 :
Flash14 :

## Menu

##

Type de carte

###

Type de Communication:

###

Son Moteur:
AIR STARTER
Air starter Sound:
VOLUME:
Start Idle Stop Starter Starter Stop Slow Rev Volume RPM/ACC:
RPM range RevRPM range Acceleration Deceleration

###

Mixage
Mixage Lineaire
Inv ESC
Mixage(direction/gaz) Av/Arr:

###

Gaz:
Profondeur:
Aillerons :
Derive (Direction):
Inversion Ch derive

###

Channel 1 Channel 5 Channel 9 Channel 13
Channel 2 Channel 6 Channel 10 Channel 14
Channel 3 Channel 7 Channel 11 Channel 15
Channel 4 Channel 8 Channel 12 Channel 16

###

Engine ON/OFF
CH Motor Off Time Light Off Time Radar Off Time

###

Volume Control
CH
MIN INT MAX

###

Start SounBoard Sound:
AIR_STARTER
AIR_STOP
AIR_STARTER2
AIR_STOP2
Small Diesel
Large Diesel
turbo_diesel
Diesel120HP
diesel 180 hp
Diesel
Small_diesel_tug
OldDiesel
Diesel7
V12
PT_BOAT
Small_Motor
Vapeur

###

Action 1 ( pêche/remorquage):

###### Quand est activé,Allume les feux, et quand le mode FOG est activé joue le son
"un son long suivi de deux sons brefs toutes les deux minutes"
Choix des leds allumées pdt l'action
Les sous actions sont disponible grace au switch de l'action 12 ( sequentiel 1A On/ 1A+1B On / 1A+1B+1C On/ 1A+1B on /1A On )

Action 1 Active
CH
HIGH
NEUTRAL
LOW
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Led
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Flash
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Na
On Time Off Time
Sous action1B
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Led
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Flash
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Na
Sous action1C
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Led
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Flash
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Na
Action 2 (Mouillage):

###### Quand est activé,active le moteur de l'ancre et quand le mode FOG est activé joue le son de "cloche"
"Un navire au mouillage doit émettre un tintement de cloche de 5 sectoutes les minutes"

Choix du type de bateau
Son Chaine Volume
Moteur
Speed Up Speed Down
Ancre auto
Action 2 Active
CH
HIGH
NEUTRAL
LOW
Action 3 (Fog):

###### Quand est activé," Les signaux phoniques par visibilité réduite" sont activés
ex:Un navire à moteur avec erre doit émettre un son long toutes les deux minutes
Choix des leds allumées pdt l'action

Choix du type de bateau
1 2 3 4 5 6 7 8 9 10 11 12 13 14
Action 3 Active
CH
HIGH
NEUTRAL
LOW
Short Blast Volume
Long Blast Volume
Bell Volume
Add Perso Files:
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
Sound Preview :
Bell1
LongBlast1
LongBlast1
LongBlast3
LongBlast4
LongBlast5
LongBlast6
LongBlast7
LongBlast8
LongBlast9
Action 4 (Manoeuvre):

###### Quand est activé," Les signaux phoniques de manoeuvre" sont activés
ex:Un bateau qui vire à bâbord émet deux sons brefs
Active sur la voie DERIVE
Choix des leds allumées pdt l'action

1 2 3 4 5 6 7 8 9 10 11 12 13 14 Na
Action 4 Active
CH
HIGH
NEUTRAL
LOW
Action 5 (Avertissement):

###### Quand est activé," Les signaux phoniques d'avertissement" sont activés
ex:En cas de dépassement dans un chenal étroit, le bateau rattrapant qui veut dépasser par bâbord émet deux sons longs suivis de deux sons brefs
Active sur la voie AILLERONS

Action 5 Active
CH
HIGH
NEUTRAL
LOW
Action 6 (Mitraillettes):

###### Quand est activé," Son Mitraillettes et sequence servo" "
Choix des leds allumées pdt l'action (Flash lors du tir)
Pour les sequences la position de départ des servos est définie dans l'action 12 ( Home )

1 2 3 4 5 6 7 8 9 10 11 12 13 14 Na
Action 6 Active
Manual servo
CH
HIGH
NEUTRAL
LOW
Sequence 6 active
Total Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Sequence 6b active
Total Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Choix Son Canon Anti Aerien Volume
Add Perso Files:
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
AA_Gun_Large
AA_Gun_Med
AA_Gun_Small
Action 7 (Canons):

###### Quand est activé," Son canon et sequence servo"
Choix de la led allumées pdt l'action ( flash lors du tir)
Pour les sequences la position de départ des servos est définie dans l'action 12 ( Home )

1 2 3 4 5 6 7 8 9 10 11 12 13 14 Na
Action 7 Active
Manual servo
CH
HIGH
NEUTRAL
LOW
Sequence 7 active
Total Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Sequence7b active
Total Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Start at secondes
and
Move To Duration
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Play sound
at secondes Optional end secondes
Choix Son Canon Volume
Add Perso Files:
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
Action 8 (Alarme):

###### Quand est activé," Son alarme"
Choix des leds allumées pdt l'action ( flash )

1 2 3 4 5 6 7 8 9 10 11 12 13 14
On Time Off Time
Action 8 Active
CH
2 Sounds
Manual servo
HIGH
NEUTRAL
LOW
Choix Son Alarme Volume
Choix Son Alarme2 Volume
Add Perso Files:
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
Alarm1
Alarm2
Alarm3
Alarm4
Ring
Action 9 (Lumiere):

###### Controle des lumieres
LEDS allumée automatiquements lors du demarage ou active par la voie

1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Led
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Flash
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Na
On Time Off Time
Auto Light
CH
HIGH
NEUTRAL
LOW
Action 10 :

###### Choix des leds allumées pdt l'action

1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Led
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Flash
1 2 3 4 5 6 7 8 9 10 11 12 13 14 /Na
On Time Off Time
Action 10 Active
Manual servo
CH
HIGH
NEUTRAL
LOW
Action 11 : Play Sound
Action 11 Active
Action 11A Active
CH
HIGH Repeat
NEUTRAL Repeat
LOWRepeat
Action 11B Active
CH
HIGHRepeat
NEUTRALRepeat
LOWRepeat
Action 11C Active
CH
HIGHRepeat
NEUTRALRepeat
LOWRepeat
Action 11D Active
CH
HIGHRepeat
NEUTRALRepeat
LOWRepeat
Add Perso Files:
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
Seagull Volume
Ambient Volume
Eleven1 Volume
Eleven2 Volume
Eleven3 Volume
Eleven4 Volume
Eleven5 Volume
Eleven6 Volume
Eleven7 Volume
Eleven8 Volume
Action 12 : Momentray switch Servo
Toggle short : Switch servo/ action1 led
Toggle long : Action servo
Action 12 Active
Switch Act1
Switch Servo
Nbr de Servos dans le switch ( 2 servos = servo 1 et servo 2)
2 AXIS ( controle par AIL et EL)
CH
HIGH
NEUTRAL
LOW
Servo Min Servo Max
ACTION: ( toggle Long)
SERVO1 Auto home when engine Off Home servo1
SERVO2 Auto home when engine Off Home servo2
SERVO3 Auto home when engine Off Home servo3
SERVO4 Auto home when engine Off Home servo4
SERVO5 Auto home when engine Off Home servo5
SERVO6 Auto home when engine Off Home servo6
Twelve1 Volume
Twelve2 Volume
Twelve3 Volume
Add Perso Files:
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
Sequences Servo and led :
Pour les sequences la position de départ des servos est définie dans l'action 12 ( Home ) SEQUENCE 1
Sequence 1 active
Total Duration
CH
HIGH
HIGH
LOW

##### Servos

Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration

##### Continuous Servos

Start at sec
Speed Stop at
Start at sec
Speed Stop at
Start at sec
Speed stop at
Start at sec
Speed stop at
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
SEQUENCE 1B
Sequence 1 active
Total Duration

##### Servos

Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration

##### Continuous Servos

Start at sec
Speed Stop at
Start at sec
Speed Stop at
Start at sec
Speed stop at
Start at sec
Speed stop at
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
SEQUENCE 2
Pour les sequences la position de départ des servos est définie dans l'action 12 ( Home )
Sequence 2 active
Total Duration
CH
HIGH
HIGH
LOW

##### Servos

Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration

##### Continuous Servos

Start at sec
Speed Stop at
Start at sec
Speed Stop at
Start at sec
Speed stop at
Start at sec
Speed stop at
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
SEQUENCE 2B
Sequence 2B active
Total Duration

##### Servos

Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration
Start at sec
and
Move To Duration

##### Continuous Servos

Start at sec
Speed Stop at
Start at sec
Speed Stop at
Start at sec
Speed stop at
Start at sec
Speed stop at
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Start at sec
Stop at sec OnTime OffTime
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Play sound
at sec Optional end sec
Output:

### Audio Converter for AUX Sound:

###
Sound files (22'050 Hz, 8 bit PCM recommended)
Copy the file in: /sounds/boat/AuxSound/
Name: File: Output:

### bitluni's audio to header converter for Engine Sounds

Modified version for Croky_b
1. Select the export file format (it is recommended to leave the settings as they are):
normalize resample
2. Select the export file type you want (for idle, Start, Stop. sound):
3. Open the unsigned 8bit PCM, 22050Hz wav file, which was previously made with Audacity:
4. Your .h file is generated and downloaded. -> Save it in /sound/boat